{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet2","index":0,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["问","答"]
["污水处理红菌工艺是什么","“红菌”是北京排水集团科研团队对污水脱氮的主角——厌氧氨氧化菌的昵称。水务红菌工艺主要包括“红菌”技术的研发和应用，以实现高效的城市污水处理。\n具体来说，该工艺首先由排水集团挑选精兵强将组建“红菌”技术研发团队，系统地进行菌群相互作用机理、环境因子调控等一系列科学研究，自主培育出“红菌”。随后，团队加快研发速度，在国内率先突破“红菌”工程化培养瓶颈，成功打造出具有完全自主知识产权的RENOCAR“红菌”脱氮技术。\n在应用方面，“红菌”技术被广泛应用于处理复杂高氨氮废水，如湖北十堰渗滤液处理厂就建设了一条全新的垃圾渗滤液处理工艺路线，以“同步反硝化产甲烷——厌氧氨氧化”的方式实现高效除碳脱氮。此外，在城市污水处理中，“红菌”技术也显示出其优越性，处理后的中水水质得到显著改善，可用于多种用途，包括冲洗车辆、家庭冲厕所、城市园林景观浇花补水以及城市市政建设等。\n总的来说，“红菌”工艺是一种创新的城市污水处理技术，通过培养和应用“红菌”，实现污水的高效处理和资源化利用，为水务领域带来新的解决方案。"]

{"sheet":"Sheet3","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}